The terminal program for CW-operators. You can transmit both from the keyboard
and from the paddle connected to a joystick connector (or to LPT, COM...).
While operating in paddle mode iambic sending (the memory of a unit of
the symbol) is possible. The handle of the transceiver (PTT and
CW keying) is made through one of the COM, LPT or USB ports.
Can co-operate with RZ4AG AALog logger.
Windows XP/Vista/7/8/10.
 
FreeWare.

Run setup.exe to install.
You need to reboot computer after installation.
      
The program is freely distributable, but you must distribute the original
archive unmodified. 
          
Sergei Podstrigailo,
UA9OV

http://www.dxsoft.com
mailto:sp@dxsoft.com
 