 
          TrueTTY ham radio digital communications software V3.33
 
This program is designed for amateur radio digital communications via a sound
card. Supported modes are RTTY (Baudot code), ASCII (7 or 8 bits),
PSK31 (BPSK and QPSK), BPSK63, QPSK63, BPSK125, AMTOR-FEC (SITOR-B, NAVTEX),
MultiFSK-16, MultiFSK-8, PS2x5, PS33x5. 
HF-PACKET and UHF-PACKET (AX25) are supported in KISS-TNC emulation mode.
SELFEC SITOR, AMTOR-ARQ (SITOR-A), PACTOR1-FEC and DTMF code decoding is also possible. 

New experimental modes PS2x5 and PS33x5 are supported!

No additional hardware required - you need only transceiver and computer
with sound card. Optionally you can use simple circuit for PTT-control.
It make fast and convenient frequence control, has a lot macros for
transmitting. Can cooperate with RZ4AG AAlog logger.  
 
It works in Windows XP/Vista/7/8/10/11.
             
Shareware ($35 or 35 Euro).          
                     
Run setup.exe to install.
You need to be logged in as an administrator when
installing the program and you need to restart computer after installation.
 
The program is freely distributable, but you must distribute the original
archive unmodified.
                     
Sergei Podstrigailo,
UA9OV        
                      
mailto:sp@dxsoft.com
https://www.dxsoft.com 
DXsoft-Support Telegram group:  https://t.me/DXsoftSupport
